#106 Dovetail Corrugated Anchor Specification

SECTION 04 00 00 MASONRY

Section 04 05 19.16 Masonry Anchors

Section 04 05 23 Masonry Accessories

**PART 1: GENERAL**

 1.1 RELATED SECTIONS

 A. Provide shop drawings for all product locations.

 1.2 SUBMITTALS

 A. Manufacturer Certificate of Compliance for materials.

 B. Product Data: Manufacturer’s data sheet on each type of product furnished.

**PART 2: MANUFACTURER**

 2.1 MANUFACTURER

 Heckmann Building Products

 110 Richards Ave.

 Norwalk, CT 06854-1685

 800-621-4140

 Email: info@heckmannanchors.com

 Website: [www.heckmannanchors.com](http://www.heckmannanchors.com)

2.2 APPLICATIONS

1. Provide anchoring systems that comply with the Building Code Requirements for Masonry Structures TMS 402-22.

 B. Stainless Steel AISI [Type 304] [or] [Type 316]

 C. ASTM A240/A240M-15b Standard Specification for Chromium and Chromium- Nickel Stainless Steel Plate, Sheet, and Strip for Pressure Vessels and for General Application.

 D. ASTM A666-15 Standard Specification for Annealed or Cold-Worked Austenitic Stainless Steel Sheet, Strip, Plate, and Flat Bar.

2.3 MATERIALS

 *Select gauge, length and steel type*

 **106 DOVETAIL CORRUGATED ANCHOR [gauge] x 1 inch (25 mm) wide x [length from face of concrete]**

**[Type 304 Stainless Steel] or [Type 316 Stainless Steel]**

**PART 3: EXECUTION**

 A. Install as specified in applicable masonry section(s).

B. Anchors: Insert anchor at desired height into Dovetail Anchor Slot. Turn 90 degrees to lock into the slot. Place mortar above and below anchor in the mortar joint**. [Specify spacing of anchors].**