#315 Weld-On Anchor Rod

SECTION 04 00 00 MASONRY

Section 05 12 00 Structural Steel Framing

Section 04 05 19.16 Masonry Anchors

**PART 1: GENERAL**

 1.1 RELATED SECTIONS

 A. Provide shop drawings for all product locations.

 1.2 SUBMITTALS

 A. Manufacturer Certificate of Compliance for materials.

 B. Product Data: Manufacturer’s data sheet on each type of product furnished.

**PART 2: MANUFACTURER**

 2.1 MANUFACTURER

 Acceptable Manufacturer:

 Heckmann Building Products

 110 Richards Ave.

 Norwalk, CT 06854-1685

 800-621-4140

 Email: info@heckmannanchors.com

 Website: [www.heckmannanchors.com](http://www.heckmannanchors.com)

2.2 APPLICATIONS

 A. Provide anchoring systems that comply with the Building Code Requirements for Masonry Structures TMS 402-16.

 B. ASTM A1008/A1008M Sheet Metal Anchors and Ties (Plain Steel)

 C. ASTM A641/641M-09a (2014) Standard Specification for Zinc-Coated (Mill Galvanized) Carbon Steel Wire.

2.3 MATERIALS

 **NO. 315 WELD-ON ANCHOR ROD**

¼” diameter x [5” long] [9” long]

 Materials:[Plain Steel] [Mill Galvanized]

**PART 3: EXECUTION**

 A. Install as specified in applicable masonry section(s).