#585 Joist Pin Anchor

#586 Twisted Joist Pin Anchor

SECTION 04 00 00 MASONRY

Section 04 05 19.16 Masonry Anchors

**PART 1: GENERAL**

1.1 RELATED SECTIONS

A. Provide shop drawings for all product locations.

1.2 SUBMITTALS

A. Manufacturer Certificate of Compliance for materials.

B. Product Data: Manufacturer’s data sheet on each type of product furnished.

**PART 2: MANUFACTURER**

2.1 MANUFACTURER

Acceptable Manufacturer:

Heckmann Building Products

110 Richards Ave.

Norwalk, CT 06854-1685

800-621-4140

Email: info@heckmannanchors.com

Website: [www.heckmannanchors.com](http://www.heckmannanchors.com)

2.2 APPLICATIONS

A. Provide anchoring systems that comply with the Building Code Requirements for Masonry Structures TMS 402-16.

B. ASTM A653/A653M-11 Standard Specification for Steel Sheet, Zinc-Coated (Mill Galvanized)

2.3 MATERIALS

1. **NO. 585 JOIST PIN ANCHOR**

1/8” x 1” wide x [Length [14”] [18”]] with 7/32” nailing holes and a fixed 3/8” x 5” pin centered 1” from end.

1. **NO. 586 TWISTED JOIST PIN ANCHOR**

1/8” x 1” wide x [Length [14”] [18”]] with 7/32” nailing holes and a fixed 3/8” x 5” pin centered 1” from end. Twist to start [length] from end of nailing side.

Materials: [Mill Galvanized]

**PART 3: EXECUTION**

A. Install as specified in applicable masonry section(s).