#585 Joist Pin Anchor

#586 Twisted Joist Pin Anchor

SECTION 04 00 00 MASONRY

Section 04 05 19.16 Masonry Anchors

**PART 1: GENERAL**

 1.1 RELATED SECTIONS

 A. Provide shop drawings for all product locations.

 1.2 SUBMITTALS

 A. Manufacturer Certificate of Compliance for materials.

 B. Product Data: Manufacturer’s data sheet on each type of product furnished.

**PART 2: MANUFACTURER**

 2.1 MANUFACTURER

 Acceptable Manufacturer:

 Heckmann Building Products

 110 Richards Ave.

 Norwalk, CT 06854-1685

 800-621-4140

 Email: info@heckmannanchors.com

 Website: [www.heckmannanchors.com](http://www.heckmannanchors.com)

2.2 APPLICATIONS

 A. Provide anchoring systems that comply with the Building Code Requirements for Masonry Structures TMS 402-16.

B. ASTM A653/A653M-11 Standard Specification for Steel Sheet, Zinc-Coated (Mill Galvanized)

2.3 MATERIALS

1. **NO. 585 JOIST PIN ANCHOR**

1/8” x 1” wide x [Length [14”] [18”]] with 7/32” nailing holes and a fixed 3/8” x 5” pin centered 1” from end.

1. **NO. 586 TWISTED JOIST PIN ANCHOR**

1/8” x 1” wide x [Length [14”] [18”]] with 7/32” nailing holes and a fixed 3/8” x 5” pin centered 1” from end. Twist to start [length] from end of nailing side.

Materials: [Mill Galvanized]

**PART 3: EXECUTION**

 A. Install as specified in applicable masonry section(s).